Changing language on handheld BY-OBD tool  (AutoXray EZ-scan4000)

Language can be changed by uploading the different language by PC/laptop into the Ezscan4000 unit. The following languages are available:

· English (“ENG”)

· Spanish (“ESP”)

· French (“FRE”)

· German (“GER”)

· Italian (“ITA”)

· Portuguese (“POR”)

Requirements are that the USB drivers are installed and that connection is verified by EZ-PC tool

Programming the unit:

Determine which COM-port the SDL connection cable has, as follows:

Open Windows “Device Manager “, as follows:

To open Device Manager, click Start, and then click Control Panel. Click Performance and Maintenance, and then click System. On the Hardware tab, click Device Manager.

Click “Ports” and note down  the COM port number.
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Startup language programming tool “ManufTests.exe”
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Connect the interface cable to the same USB port as used earlier

Wait if driver installation sequence begins. If yes, choose automatic installation.

Windows might give following warning; Click “CONTINUE ANYWAY”
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Turn on the tool

Press CONFIG

Scroll down to “3-download”

Press Enter

Then testing of settings will begin,

Followed by programming of the tool with the required language.

1: Select desired language





2: fill in 0 (zero) to keep the same serial number





3: check this box to program the language after testsequence





4: fill in Com Port noted earlier 








