CANBus Control Head Calibration (with software > v1.09)

This calibration procedure is for Dual function single lever (both shift and throttle on a lever) controls. Controls are factory calibrated, but this procedure is supplied in the event you need to restrict CH675XX, CH676XX, CH1900 or travel.

SINGLE CONTROL HEAD

Single lever – Single Engine Controls

· With the system OFF (no power on the CANBus) press and hold the N (NEUTRAL) button on the control head and turn the power ON. The Neutral lamp will blink.

· Move the lever to the FULL FORWARD position. The Neutral lamp will blink. Press the SELECT button. The Select lamp will turn on.

· Move the lever to the FORWARD IDLE position. The Neutral lamp will blink. Press the SELECT button. The Select lamp will turn on.

· Move the lever to the NEUTRAL position. The Neutral lamp will blink. Press the SELECT button. The Select lamp will turn on.

· Move the lever to the REVERSE IDLE position. The Neutral lamp will blink. Press the SELECT button. The Select lamp will turn on.

· Move the lever to the FULL REVERSE position. The Neutral lamp will blink. Press the SELECT button. The Select and Neutral lamps will both blink indicating the process is complete. Turn the power OFF to exit the calibration process.

DUAL or TRIPLE CONTROL HEAD

PORT Lever - Dual or Triple engine Controls

· With the system OFF (no power on the CANBus) press and hold the PORT N (NEUTRAL) button on the control head and turn the power ON. The port Neutral lamp will blink.

· Move the Port lever to the FULL FORWARD position. The port Neutral lamp will blink. Press the SELECT button. The Select lamp will turn on.

· Move the Port lever to the FORWARD IDLE position. The port Neutral lamp will blink. Press the SELECT button. The Select lamp will turn on.

· Move the Port lever to the NEUTRAL position. The port Neutral lamp will blink. Press the SELECT button. The Select lamp will turn on.

· Move the Port lever to the REVERSE IDLE position. The port Neutral lamp will blink. Press the SELECT button. The Select lamp will turn on.

· Move the Port lever to the FULL REVERSE position. The port Neutral lamp will blink. Press the SELECT button. The Select and port Neutral lamps will both blink indicating the process is complete. Turn the power OFF to exit the port calibration process.

STARBOARD (STB) Lever - Dual or Triple engine Controls

· With the system OFF (no power on the CANBus) press and hold the STB N (NEUTRAL) button on the control head and turn the power ON. The STB Neutral lamp will blink.

· Move the STB lever to the FULL FORWARD position. The STB Neutral lamp will blink. Press the SYNC button. The Select lamp will turn on.

· Move the STB lever to the FORWARD IDLE position. The STB Neutral lamp will blink. Press the SYNC button. The Select lamp will turn on.

· Move the STB lever to the NEUTRAL position. The STB Neutral lamp will blink. Press the SYNC button. The Select lamp will turn on.

· Move the STB lever to the REVERSE IDLE position. The STB Neutral lamp will blink. Press the SYNC button. The Select lamp will turn on.

· Move the STB lever to the FULL REVERSE position. The STB Neutral lamp will blink. Press the SYNC button. The Select and STB Neutral lamps will both blink indicating the process is complete. Turn the power OFF to exit the Starboard (STB) calibration process.

