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Updating with Web updater 1.3:
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After clicking “Next”, Contact is made via internet to update program

Several screens indicate several parts of the program are updated
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New version
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Files stored in following dir.:

C:\Program Files\AutoXray\EZ-PC\data\*.psc

Downloading data collected by tool, using “Scan” and “MON-Capture” menu’s

Open EZ-PC, Go to menu Tool Link – Get data from tool
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Follow instructions below




Get tool data:
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Three windows will pop up:


[image: image9.png]¥ Fle_Software Update  Tool Link Help
Cascade

Tie
biaGNOSTICS BY. Arrange Icons

v 1 Scan Report
2 Capture Data (List)
3 Capture Data (Graph)






Scan report is ready to print:
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Vehicle Scan Report
Data Downloaded from Scanner: 08/27/2007 02:57 PM

Comments

testresult in testcell

Trouble Codes

P0222 Throttle / Pedal Position Sensor / Switch B Circuit Low Input
P0122 Throttle/Pedal Position Sensor/Switch A Circuit Low Input
U0001 High Speed Controller Area Network Communication Bus
PO650 Malfunction Indicator Lamp (MIL) Control Circuit Malfunction

Pending Codes

P0222 Throttle / Pedal Position Sensor / Switch B Circuit Low Input
P0122 Throttle/Pedal Position Sensor/Switch A Circuit Low Input
U0001 High Speed Controller Area Network Communication Bus
PO650 Malfunction Indicator Lamp (MIL) Control Circuit Malfunction

Freeze Frame Codes
POBS0 Malfunction Indicator Lamp (MIL) Control Circuit Mafunction

Readiness Test Results

MIL Status orf

Misfire Monitor Not Supported
Fuel System Monitor Not Supported
Comprehensive Component Completed
Catalyst Not Supported
Heated Catalyst Not Supported

Operational Data

Evaporative System
Secondary Alr System
AIC Refrigerant

02 Sensor

02 Sensor Heater
EGR System

# Parameter Name Value Units (if applicable)

1 Readiness Monitors Complete Yes

2 Load Value 0.00 %

3 Coolant Temp 86.00 c

4 MAP Sensor 10200 kPa

5 Engine RPM 0.00 RPM

6 Venicle Speed 0.00 kmin

7 Intake Air Temp 33.00 c

8 Air Flow Rate 0.00 gmisec

9 OBD Il Require Not Intended

10 Fuel rail pressure (gauge) 6500 0kPa
Freeze Frame Data

# Parameter Name Value Units (if applicable)

1 Load Value 0.00 %

2 Coolant Temp 83.00 c

3 MAP Sensor 101.00 kPa

4 Engine RPM 0.00 RPM

5 Vehicle Speed 000 Kkmin

www.autoxray

Not Supported
Not Supported
Not Supported
Not Supported
Not Supported
Not Supported





Capture data list as follows
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Parameter Name [ [ [ [ B} 1 H G
Readiness Monitors Complete (Yes=0) O [ [ [ [ 0 0 0
Load Value (%) 000 000 000 000 000 000 000 000
Coolant Temp (°C) 84,00 84,00 84,00 84,00 84,00 84.00 84.00 84.00
AP Sensor (kPa) 102,00 102,00 102,00 102,00 102,00 102.00 102.00 102.00
Engine RPM (RPHM) 000 000 000 000 000 0.00 0.00 0.00
vehicle Speed (kmfh) 000 000 000 000 000 0.00 0.00 0.00
Intake Ar Temp (°C) 37.00 37.00 37.00 37.00 37.00 37.00 37.00 37.00
Air Flow Rate (gm/sec) 000 000 000 000 000 0.00 0.00 0.00
OBD I1 Require (Not Intended=0) 0 0 0 0 0 i i i

Fuel rail pressure (gauge) (0 kPa) 43.00 43.00 43.00 43.00 43.00 43.00 43.00 43.00




These data can be exported to a .CSV file (Comma delimited file, can be opened with Excel)
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Opening in Excel gives following result:
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To convert, select first column, and go to menu “Data-Text to Columns”
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Select “Delimited”
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Select “Comma”, and click finish
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Result as follows:
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In Capture data (graph) window, data can be viewed and printed.
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